APPX “E”

PRICE BID FORMAT FOR CARRYING OUT OF WORK FOR RENOVATION/UPGRADATION OF EXISTING CLASSROOMS

The price bid format is given below and bidders are required to fill this up correctly with full details. Failure to provide details will render bid invalid. (Please attach detail specification on attached sheet)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **SER NO** | **Particulars** | **SPECIFICATION** | **QTY** | **BASIC COST** | **GST** | **TOTAL (IN FIGURE)** | **TOTAL (IN WORDS)** |
| 1 | Repairing Ceiling | Non asbestos 4mm thick along with necessary bidding | 120 Sqm |  |  |  |  |
| 2 | Frames for ceiling | Fixing of wooden frame works for the ceiling | 120 Sqm |  |  |  |  |
| 3 | Painting of ceiling | Prime Coat & Distemper | 120 Sqm |  |  |  |  |
| 4 | Wall paneling | Panelling of all walls of nine classrooms with 6 mm ply | 405 Sqm |  |  |  |  |
| 5 | Frame work for the wall | Making of wooden frame work for doing the wall panelling with 6 mm ply | 405 Sqm |  |  |  |  |
| 6 | Painting | Synthetic painting of panelling along with prime coat | 405 Sqm |  |  |  |  |